|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S. NO.** | **DESCRIPTION** | **UNIT** | **QTY.** | **Rates** | **AMOUNT** | Make / Brand |
| **PART A.** | **PIPING MAIN / RISERS** |  |  |  |  |  |
| 1 | Providing and fixing **M.S. pipe** to I.S. 1239 (Heavy class) complete with painting with one coat of primer after surface preparartion and two coats of synthetic enamel paint, cutting and making good the walls good complete. Pipe upto 50 mm dia threaded joints with holdtite, 50 mm dia and above should be welded joint (all type) (internal works/External Works) |  |  |  |  | Jindal / Tata ISI marked |
| b. | 100mm dia | Mtrs | 6 |  |  |  |
| 2 | Supply & Installation of MS class heavy bents by means of welding including painting One coat of red oxide & Two coat of PO red enamel paint | Nos | 5 |  |  |  |
| 3 | Charges for Cutting & removing Old pipe from location by means of Cutting with Welding machine / Electric cutter & placing pipe in Open area outside the building including making holes in the Brick wall & Holes in the FHC box for removing the pipe & laying new one indluding Removing of Existing HYdrant landing valves & HOse reel & Re connection of same on new pipe. | Lumpsump | 1 |  |  |  |
| 4 | Dismantling & Remaking of False ceiling with aluminium channel & required Gypsum board with Painting & with Cutting for Re-fitting of Elec. Light | Sq.ft | 55 |  |  |  |
| 5 | Supply of C.I. **butterfly valves** Lever type PN 1.6 complete with bolts, nuts 1.5mm thick compressed asbestos gasket companion flanges complete. 100 mm Dia Size. (On the floor) | Nos | 1 |  |  |  |
| 6 | Providing & fixing of MS support / Hamger made of 35 X 35 X 5 mm size angle with required fastners, MS plate etc complete in all respect with painting One coat of Red oxide & Two coat of PO red enamel paint. | Nos | 2 |  |  |  |
|  | **Grand Total** |  |  |  |  |  |
|  |  |  |  |  |  |  |

* Total Cost of work: \_\_\_\_\_\_\_\_\_
* GST: \_\_\_\_\_\_\_\_\_
* Time required for completion of work: \_\_\_\_\_\_\_\_\_
* Validity of this quotation: \_\_\_\_\_\_\_\_\_

Signature: \_\_\_\_\_\_\_\_\_

Name: \_\_\_\_\_\_\_\_\_\_\_\_

Seal: \_\_\_\_\_\_\_\_\_\_\_\_\_

Interested contractors are requested to visit the site before submitting their quotes.

The quote should be inclusive of all charges i.e. the cost of material, tools, labour, transport etc. GST should be quoted separately.

For site visit and any further clarifications, you may visit ICGEB on any working day (Monday to Friday) between 9.30 a.m. to 5 p.m. (contact person Mr. Varun).

Quotations should be submitted in a sealed envelope, clearly marked as **‘ND quotation for work at ICGEB, New Delhi Component 02(R)/2019’**. Kindly ensure that this identification number is also mentioned on the quotation. The sealed envelope, with the quotation, should bear the official stamp of the bidder, both on front of the envelope and across the seal of the envelope. The sealed envelope with the quotation should be placed in a further sealed envelope and submitted to:

The Component Manager

ICGEB

Aruna Asaf Ali Marg

New Delhi – 110 067

**The quotation should be submitted latest by Wednesday, 27th March, 2019**