**CORRIGENDUM:**

Please find below the changes in financial bid and scope of work (mark in red colour)

**FINANCIAL BID**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***No.*** | ***Description*** | ***Unit*** | ***Quantity*** | ***Unit Rate*** | ***Amount.*** |
|  | **False Ceiling Work** |  |  |  |  |
| **1** | **Providing & fixing false ceiling at all height including providing & fixing of framework made of special section, power pressed from M.S. sheets and galvanized with zinc coating of 120 gms/ sqm (both side inclusive) as per IS : 277 and consisting of angle cleat of size 25mm wide x 1.6mm thick with flanges of 27mm and 37mm, at 1200mm c/c, one flange fixed to the ceiling with dash fastener 12.5mm dia x 50mm long with 6mm dia bolts, other flange of cleat fixed to the angle hangers of 25 x10 x0.50mm of required length with nuts & bolts of required size and other end of angle hanger fixed with intermediate G.I channels 45 x15 x 0.90mm running at the spacing of 1200 mm c/c, to which the ceiling section 0.5mm thick bottom wedge of 80mm with tapered flanges of 26 mm each having lips of 10.5mm, at 450mm c/c, shall be fixed in a direction perpendicular to G.I intermediate channel with connecting clip made out of 2.64mm dia x 230mm long G.I wire at every junction, including fixing perimeter channels 0.50mm thick 27mm high having flanges of 20mm and 30mm long, the perimeter of ceiling fixed to wall/ partitions with the help of Rawl plugs at 450mm center, with 25mm long dry wall screws @ 230mm interval, including fixing of (Make)Calcium Silicate Board to ceiling section and perimeter channels with the help of dry wall screws of size 3.5 x25mm at 230mm c/c, including jointing & finishing to a flush finish of tapered and square edges of the board with recommended jointing compounds, jointing tapes, finishing with jointing compounds in three layers covering up to 150mm on both sides of joints and two coats of primer suitable for boards, all as per manufacture's specification and also including the cost of making opening for light fittings, grills, diffusers, cut outs made with frame of perimeter channels suitably fixed, all complete as per drawings, specification and direction of the Engineer in charge but excluding the cost of painting with: Note: False Ceiling will be as per details provided in detail drawings and vertical strips will be measured and counted along with horizontal strips for this items a. 8 mm thick Calcium Silicate Board made with Calcareous & Siliceous materials reinforced with cellulose fiber manufactured through autoclaving process and plastic emulsion paint as required** | **SFT** | **850** |  |  |
| **2** | **Repair, Extension and Re installation of Duct** | **Lump Sum** | **1** |  |  |
| **3** | **Providing and installation of Polyvinyl Flooring of LG Delite 2.2 mm Make / Equi.** | **SFT** | **850** |  |  |
| **4** | **Wooden covering of 350 mm X100 MM for Drain Pipe of AC** | **RFT** | **350** |  |  |
| **5** | **Supply and Installation of Powder Coated Diffuser of size 600mm x 6000mm complete with all connection of Green Air Make.** | **N0** | **2** |  |  |
| **6** | **Supply and Installation of LED surface finish light of 4000 K with 36 W of 600 MMX600 MMon ceiling of WIPRO / Havell Make.** | **No** | **16** |  |  |
| **7** | **Supply and Installation. Work of preparation of wall surface for panting including removing the existing puffed/ damaged old paint surface, applying birla putty two coats, finishing the wall surface with emery paper applying primmer one coats and then application of plastic emulsion paint in two coats for finished wall** | **Sq.ft** | **1000** |  |  |
|  |  |  |  |  |  |
|  | **TOTAL** |  |  |  |  |
|  |  |  |  |  |  |